# IEEE Guide for bus design in air insulated substations

## Proposed tutorial plan - version 1

### September 26, 2012

## Objectives

* Familiarize the substation engineer with the design process of flexible and rigid bus design
* Familiarize the substation engineer with the different calculation methods available for bus design: from hand on calculations to finite element calculations; provide an overview of the advantages and limitations of these.

## Details

* Duration : 8 hours
* Instructors: Hanna Abdallah (HA) and Jean-Bernard Dastous (JBD)

## Content and schedule

|  |  |  |  |
| --- | --- | --- | --- |
| item# | Subject | Instructor | Duration(minutes) |
| 1 | Overview, Scope and purpose of 605.  | HA | 15 |
| 2 | Main changes/improvements from IEEE-605-1998 | HA | 15 |
| 3 | Differences between 605 and ASCE 113 Substation Structure Design Guide | JBD | 15 |
| 4 | Overview of the design procedure:* General design flowchart
* Bus arrangements available: advantages and limitations
* Construction types available : advantages and limitations
* Design considerations
* Conductors
 | HA | 60 |
| 5 | Bus ampacity calculations and annexes B and C of the guide | HA | 30 |
| 6 | Corona and annex D of the guide | HA | 20 |
| 7 | Mechanical Design:* General design procedure
* Load evaluations : gravity, wind, ice, short-circuit, thermal
* Calculation methods : hand on and finite-element calculation
* Comparison between hands on and finite element calculations for short-circuit loading
* Acceptance criteria: maximum allowable span, strength of porcelain, vibration attenuation
 | JBD | 75 |
| 8 | Design example #1: Rigid bus design | HA/JBD | 90 |
| 9 | Design example #2: Strain bus design | HA/JBD | 90 |